<Huawei>

Nov 12 2022 10:12:39-08:00 Huawei %%01IFPDT/4/IF\_STATE(l)[0]:Interface GigabitEt

hernet0/0/1 has turned into UP state.

<Huawei>sys

Enter system view, return user view with Ctrl+Z.

[Huawei]sys R1

[R1]int g0/0/1

[R1-GigabitEthernet0/0/1]undo shutdown

Info: Interface GigabitEthernet0/0/1 is not shutdown.

[R1-GigabitEthernet0/0/1]q

[R1]

[R1]

[R1]

[R1]int g0/0/1.1

[R1-GigabitEthernet0/0/1.1]vlan-type dot1q 10

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]vlan-type dot1q 10

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]

[R1-GigabitEthernet0/0/1.1]

[R1-GigabitEthernet0/0/1.1]

[R1-GigabitEthernet0/0/1.1]

[R1-GigabitEthernet0/0/1.1]vlan-type

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]vlan-type 10

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]vlan-type 801.1q 10

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]q

[R1]

[R1]

[R1]vlan batch 10 20

Info: This operation may take a few seconds. Please wait for a moment...done.

[R1]int g0/0/1.1

[R1-GigabitEthernet0/0/1.1]vlan-type dot1q 10

^

Error: Unrecognized command found at '^' position.

[R1-GigabitEthernet0/0/1.1]dot1q ter

[R1-GigabitEthernet0/0/1.1]dot1q termination vid 10

[R1-GigabitEthernet0/0/1.1]ip add 192.168.10.1 24

Nov 12 2022 10:26:26-08:00 R1 %%01IFNET/4/LINK\_STATE(l)[1]:The line protocol IP

on the interface GigabitEthernet0/0/1.1 has entered the UP state.

[R1-GigabitEthernet0/0/1.1]q

[R1]

[R1]

[R1]

[R1]

[R1]int g0/0/1.2

[R1-GigabitEthernet0/0/1.2]dot1q termination vid 20

[R1-GigabitEthernet0/0/1.2]ip add 192.168.20.1 24

Nov 12 2022 10:26:51-08:00 R1 %%01IFNET/4/LINK\_STATE(l)[2]:The line protocol IP

on the interface GigabitEthernet0/0/1.2 has entered the UP state.

[R1]int g0/0/1.1

[R1-GigabitEthernet0/0/1.1]arp broadcast enable

[R1-GigabitEthernet0/0/1.1]int g0/0/1.2

[R1-GigabitEthernet0/0/1.2]arp broadcast enable

[R1-GigabitEthernet0/0/1.2]

封装vlan后开启arp广播

S1

<Huawei>sys

Enter system view, return user view with Ctrl+Z.

[Huawei]undo inf en

Info: Information center is disabled.

[Huawei]sys S1

[S1]

[S1]

[S1]vlan batch 10 20

Info: This operation may take a few seconds. Please wait for a moment...done.

[S1]int e0/0/2

[S1-Ethernet0/0/2]port link-type access

[S1-Ethernet0/0/2]port de

[S1-Ethernet0/0/2]port default vlan 10

[S1-Ethernet0/0/2]q

[S1]

[S1]

[S1]

[S1]int e0/0/3

[S1-Ethernet0/0/3]port link-type access

[S1-Ethernet0/0/3]port default vlan 20

[S1-Ethernet0/0/3]int g0/0/1

[S1-GigabitEthernet0/0/1]port link-type trunk

[S1-GigabitEthernet0/0/1]porttrunk allow-pass vlan all

^

Error: Unrecognized command found at '^' position.

[S1-GigabitEthernet0/0/1]port trunk allow-pass vlan all

